

Manual how to install the firmware.

Don't install the firmware over wireless connection, please install it over a LAN connection.


Installation of the Firmware:
- start the Webbrowser
- call the Web User Interface if the Router (Standard is http://192.168.0.1)
- on the top click on "Tools"
- on the left click on "Firmware"
- click on the button "Search"
- chose the unpacked firmware file (DIR645A1_FW102B11.bin)
- click on "Upload"

- The upgrade takes around 5 minutes, as soon as it is ready the start screen of the Web UI of the router appears.
