Bug Fixes:

1. Fixed the issue where the flash logs disappears after system reboot.
2. Removed “Refresh” button from FLASH log page.
3. Fixed the issue where the following optional TLV values of LLDP-MED are incorrect:
   Optional Mau Type
   Auto-negotiation advertised capability
   Maximum Frame size
   Asset ID
   Manufacturer name
   Firmware and Hardware revision
4. Fixed the issue where the HTTPS/SSL certificate files failed to download to the device, if it containedCR/LF control characters.

Known issues:

- Port PVID (Switching > VLAN > Advanced > Port PVID Configuration) does not automatically changed back to 1 after its associated VLAN is deleted.
  Workaround: Manually change the PVID back to 1.

Limitations:

- Combined MAC and IP ACL do not work with double VLAN tagged traffic.

Upgrade Instructions:

- Using the Download Link below, download and extract the new firmware to a convenient place such as your desktop. The filename after extracting is GS108Tv2_GS110TP_V5.4.2.25.stk
  Download Link: http://www.downloads.netgear.com/files/GDC/GS110TP/GS108Tv2_GS110TP_V5.4.2.25.zip
- Please follow the instructions provided in Upgrading GS108Tv2 and GS110TP from 5.0.1.x to 5.0.2.x to upgrade the firmware.

This product includes software code developed by third parties, including software code subject to the GNU General Public License ("GPL") or GNU Lesser General Public License ("LGPL"). As applicable, the terms of the GPL and LGPL, and information on obtaining access to the GPL Code and LGPL Code used in this product, are available to you at NETGEAR's Open Source Code Web page. The GPL Code and LGPL Code used in this product is distributed WITHOUT ANY WARRANTY and is subject to the copyrights of one or more authors. For details, see the GPL Code and LGPL Code for this product and the terms of the GPL and LGPL.