Security Fixes:

- Various security vulnerability fixes and enhancements.

Known Issues:

- Port PVID (Switching > VLAN > Advanced > Port PVID Configuration) does not automatically change back to 1 after its associated VLAN is deleted.
  Workaround: Manually change the PVID back to 1.
- Combined MAC and IP ACL do not work with double VLAN tagged traffic.

Download Link: https://www.downloads.netgear.com/files/GDC/GS110TP/GS108Tv2_GS110TPv2_V5.4.2.36.zip

Firmware Upgrade Instructions:

To update your product’s firmware, follow the instructions in your product’s user manual. To find your user manual, visit https://www.netgear.com/support/, enter your model number in the search box, and click the Documentation button on the product page.