ReadyNAS OS V6.7.2 Release Notes.

RN102 & RN104 systems running firmware older than 6.2.1 should first update to 6.2.5, then update from 6.2.5 to 6.7.2.
RN2120 systems running firmware older than 6.2.1 should first update to 6.2.4, then update from 6.2.4 to 6.7.2.
All other systems can update directly to 6.7.2.

For instructions on updating your firmware, see the ReadyNAS OS 6: Updating Firmware article.

Download Link:

arm (RN102 / RN104 / RN202 / RN204 / RN212 / RN214 / RN2120)
x86_64 (RN312 / RN314 / RN316 / RN422 / RN424 / RN516 / RN524X / RN526X / RN528X / RN626X / RN628X / RN716X / RN3130 / RN3138 / RN3220 / RN4220 / RR3312 / RR4312X / RR4312S / RR4360X / RR4360S)

The following are some items to look forward to in 6.7.2:

Bug Fixes:

- Fixes the ReadyNAS OS 6.7.1 issue with RN4220 that 10G SFP+ network card does not work