ReadyNAS OS V6.8.1 Release Notes.

For instructions on updating your firmware, see the ReadyNAS OS 6: Updating Firmware article.

The following are some items to look forward to in 6.8.1:

Bug Fixes:

- Fixed NAS discoverability in the Computers section of the network browser on recent Windows 10 versions.
- Fixed premature Out-of-Space errors in some cases.
- Fixed Update button functionality for install apps.
- Fixed SMB access from some Linux clients when the "Enhance macOS" option is enabled. (RN10x / 20x / 21x / 2120)
- Fixed UPS communication error alerts when disk spin down is enabled.
- Fixed app installation for apps with a large number of dependencies.
- Fixed an issue where backup jobs for home folders would also back up snapshots if Visible Snapshots was enabled.
- Fixed RAID 10 sync completion percentage calculation.
- Fixed visible snapshot access on NFS shares with IP address restrictions.
- Removed ReadyCLOUD access attempts to retired server.
- Relaxed handling of bad iSCSI initiator commands with sync policy set to disabled.
- Fixed iSCSI access issues on VLAN virtual interfaces associated with bond interfaces.
- Fixed management UI crash with >7 network interfaces (including VLAN interfaces).
- Fixed an issue where the bonding mode would be reset after reboot when changing to Round Robin mode.
- Fixed some installed 3rd-party apps (including Plex) not appearing in the GUI.
- Fixed a rare issue where disks 2 and 4 may drop out. (RN3130 / RN3138)

Warnings:

- Unless you are advised by NETGEAR Support in a support case to update to beta software, NETGEAR Support may deny support if you are running beta software. You can seek help here on the NETGEAR Community for issues encountered on the beta.
- Devices updated with 6.8.1 firmware should not be downgraded to firmware versions before 6.8.0.
- ReadyNAS 102, 104, and 2120 must not be updated directly to 6.8.x from 6.3.x or older firmware. They must first be updated to either 6.2.5 or 6.3.5 then to 6.5.2 and then onto 6.8.x.
- ReadyNAS 202, 204, 212 and 212 must not be updated directly to 6.8.x from 6.3.x. They must first be updated to 6.3.5 then 6.5.2 and then onto 6.8.x.

Download Link:

arm (RN102 / RN104 / RN202 / RN204 / RN212 / RN214 / RN2120)
x86_64 (RN312 / RN314 / RN316 / RN422 / RN424 / RN426 / RN516 / RN524X / RN526X / RN528X / RN626X / RN628X / RN716X / RR2304 / RN3130 / RN3138 / RN3220 / RN4220 / RR3312 / RR4312X / RR4312S / RR4360X / RR4360S)