ReadyNAS OS V6.9.2 Release Notes:

Download Link:

arm (RN102 / RN104 / RN202 / RN204 / RN212 / RN214 / RN2120)
x86_64 (RN312 / RN314 / RN316 / RN422 / RN424 / RN426 / RN516 / RN524X / RN526X / RN528X / RN626X / RN628X / RN716X / RR2304 / RN3130 / RN3138 / RN3220 / RN4220 / RR3312 / RR4312X / RR4312S / RR4360X / RR4360S)

To install: Click on appropriate link above for your system to download firmware image. Then upload that image from the management UI's System->Settings->Update->Install Firmware section.

Changelog:

- Updated kernel to fix Meltdown vulnerability (CVE-2017-5754).
- Updated several OS packages with latest security fixes.
- Added dual-boot support to handle bad NAND blocks on flash. (RN202 / 204 / 212 / 214)

Warnings:

- Devices updated with 6.9.2 firmware should not be downgraded to firmware versions before 6.9.0.
- ReadyNAS 102, 104, and 2120 must not be updated directly to 6.9.x from 6.3.x or older firmware.They must first be updated to either 6.2.5 or 6.3.5 then to 6.5.2 and then onto 6.9.x.
- ReadyNAS 202, 204, 212 and 212 must not be updated directly to 6.9.x from 6.3.x. They must first be updated to 6.3.5 then 6.5.2 and then onto 6.9.x.