# GS110TP & GS108Tv2 Firmware Version 5.4.2.11

New Features:

- Added IPv6 management, IPv6 ACL, and IPv6 DiffServ support.

Bug Fixes:

- Fixed the issue that SCCD (Smart Control Center Discovery) Utility cannot discover the device when its DHCP lease time has expired.
- Fixed the issue that VLAN does not change via RADIUS VLAN assignment unless bring the link down and up.

Known issues:

- Port PVID (Switching > VLAN > Advanced > Port PVID Configuration) does not automatically changed back to 1 after its associated VLAN is deleted.
  Workaround: Manually change the PVID back to 1.

Limitations:

- Combined MAC and IP ACL do not work with double VLAN tagged traffic.

Upgrade Instructions:

- Download and extract the new firmware to a convenient place such as your desktop.
- Please follow the instructions provided in Upgrading GS108Tv2 and GS110TP from 5.0.1.x to 5.0.2.x to upgrade the firmware.

This product includes software code developed by third parties, including software code subject to the GNU General Public License ("GPL") or GNU Lesser General Public License ("LGPL"). As applicable, the terms of the GPL and LGPL, and information on obtaining access to the GPL Code and LGPL Code used in this product, are available to you at NETGEAR's Open Source Code Web page. The GPL Code and LGPL Code used in this product is distributed WITHOUT ANY WARRANTY and is subject to the copyrights of one or more authors. For details, see the GPL Code and LGPL Code for this product and the terms of the GPL and LGPL.