ReadyNAS OS V6.10.5 Release Notes:

Download Link:

arm (RN102 / RN104 / RN202 / RN204 / RN212 / RN214 / RN2120)
x86_64 (RN312 / RN314 / RN316 / RN422 / RN424 / RN426 / RN516 / RN524X / RN526X / RN528X / RN626X / RN628X / RN716X / RR2304 / RN3130 / RN3138 / RN3220 / RN4220 / RR3312 / RR4312X / RR4312S / RR4360X / RR4360S)

Bug Fixes:

- ClamAV fails to update database.
- Replicate keeps running even after the service is disabled.
- Root partition runs out of space when audit option is enabled for shares.
- Egnyte APT repository trusted key expires.
- Readynasd service crashes while parsing authorized replicate keys.

Security Fixes:

- Fixes security issues

This firmware addresses security vulnerabilities. For more information about security vulnerabilities, visit https://www.netgear.com/about/security.

Warnings:

- Devices updated with 6.10.5 firmware should not be downgraded to firmware versions before 6.10.0.
- ReadyNAS 102, 104, and 2120 systems must not be updated directly to 6.10.x from 6.3.x or older firmware. They must first be updated to either 6.2.5 or 6.3.5 then to 6.5.2 and then to 6.10.x.
- ReadyNAS 202, 204, 212 and 212 systems must not be updated directly to 6.10.x from 6.3.x. They must first be updated to 6.3.5 then 6.5.2 and then to 6.10.x.

Firmware Update Instructions:

For instructions on updating your firmware, see https://kb.netgear.com/app/answers/detail/a_id/26212/~/readynas-os-6%3A-updating-firmware.